Example text log file |

PassMark BurnInTest Log file - http://www.passmark.com ======================================================== Date: 12/15/08 14:52:05 BurnInTest V6.0 Pro 1000 Customer: ian

Technician: tom

Logging detail level: Normal

**************

SYSTEM SUMMARY

**************

Windows XP Professional Service Pack 3 build 2600 (32-bit),

1 x Genuine Intel(R) CPU @ 2.40GHz,

2.0GB RAM,

NVIDIA Quadro FX 1400, ATI Radeon HD 3450,

149GB HDD, 75GB HDD,

CD/DVDRW,

GENERAL

System Name: XW6400XP32

System Model: HP xw6400 Workstation

Motherboard Manufacturer: Hewlett-Packard

Motherboard Name: 0A04h

Motherboard Serial Number: SAS1044ze2

BIOS Manufacturer: Hewlett-Packard

BIOS Version: 786D4 v02.26

BIOS Release Date: 09/21/2007

CPU

CPU manufacturer: GenuineIntel

CPU Type: Genuine Intel(R) CPU @ 2.40GHz

Physical CPU's: 1

Cores per CPU: 4

Hyperthreading: Not capable

CPU features: MMX SSE SSE2 SSE3 SSSE3 DEP PAE Intel64 VMX

Clock frequencies:

Measured CPU speed: 2353.8 MHz

Multiplier: x9.0

Scalable Bus Speed: 266.0 MHz

Front Side Bus: 1066.0 MHz

Cache per CPU package:

L1 Instruction Cache: 4 x 32 KB

L1 Data Cache: 4 x 32 KB

L2 Cache: 2 x 4096 KB

MEMORY

Total Physical Memory: 2047MB

Available Physical Memory: 1232MB

Memory devices:

DIMM01:

- DDR2 FB-DIMM, 2048MB, 667MHz,

- Serial number: F29F0812

DIMM02:

- Not populated

DIMM03:

- Not populated

DIMM04:

- Not populated

SYSTEM ROM:

- Flash, 33MB,

Virtual memory: C:\pagefile.sys (allocated base size 1000MB)

GRAPHICS

NVIDIA Quadro FX 1400

Chip Type: Quadro FX 1400

DAC Type: Integrated RAMDAC

Memory: 128MB

BIOS: Version 5.41.02.17.24

Driver provider: NVIDIA

Driver version: 6.14.11.6996

Driver date: 5-26-2008

Monitor 1: 1280x1024x32 60Hz (Primary monitor)

ATI Radeon HD 3450

Chip Type: ATI display adapter (0x95C5)

DAC Type: Internal DAC(400MHz)

Memory: 512MB

BIOS: 113-AAXXXXX-XXX

Driver provider: ATI Technologies Inc.

Driver version: 8.451.0.0

Driver date: 12-20-2007

Monitor 2: 1280x1024x32 60Hz

DISK VOLUMES

C: Local drive, NTFS, (74.53GB total, 7.71GB free)

E: Optical drive, TEST_DVD, CD/DVDW SH-W162Z, UDF

F: Local drive, Backup, NTFS, (139.28GB total, 2.24GB free)

K: Local drive, test, NTFS, (0.49GB total, 0.48GB free)

L: Local drive, New Volume, NTFS, (1.95GB total, 1.84GB free)

M: Local drive, New Volume, NTFS, (1.95GB total, 1.94GB free)

DISK DRIVES

Disk drive: Model ST3160827AS (Size: 149.05GB)

Disk drive: Model WDC WD800JD-60LSA0 (Size: 74.53GB)

OPTICAL DRIVES

E: TSSTcorp CD/DVDW SH-W162Z (CD/DVDRW)

NETWORK

Broadcom NetXtreme Gigabit Ethernet

PORTS

Communications Port: COM1 - RS232 Serial Port (max Baud rate: 115200)

Parallel port: LPT1

Keyboard Port: PS/2 connector

Mouse Port: PS/2 connector

Intel(R) 631xESB/6321ESB USB Universal Host Controller - 2688

Intel(R) 631xESB/6321ESB USB Universal Host Controller - 2689

Intel(R) 631xESB/6321ESB USB Universal Host Controller - 268A

- Microsoft Natural® Ergonomic Keyboard 4000

- Kensington USB/PS2 Wheel Mouse

Intel(R) 631xESB/6321ESB USB Universal Host Controller - 268B

Intel(R) 631xESB/6321ESB USB2 Enhanced Host Controller - 268C

******************

DETAILED EVENT LOG

******************

LOG NOTE: 2008-12-15 14:52:05, Status, PassMark BurnInTest V6.0 Pro 1000

LOG NOTE: 2008-12-15 14:52:06, Status, Main Tests started

LOG NOTE: 2008-12-15 14:52:06, CPU, 3DNow! SSE4.1 SSE4.2 SSE4a test(s) selected, but CPU feature not detected

LOG NOTE: 2008-12-15 14:53:08, Status, Test run stopped

**************

RESULT SUMMARY

**************

Test Start time: Mon Dec 15 14:52:05 2008

Test Stop time: Mon Dec 15 14:53:07 2008

Test Duration: 000h 01m 02s

Test Name Cycles Operations Result Errors Last Error

2D Graphics 0 275 PASS 0 No errors

CPU 11 36.701 Billion PASS 0 No errors

Disk (C: ) 0 563 Million PASS 0 No errors

Memory (RAM) 5 5.362 Billion PASS 0 No errors

Network 1 1 8640 PASS 0 No errors

Optical disk (E:) 1 25.285 Million PASS 0 No errors

Sound 0 970200 PASS 0 No errors

TEST RUN PASSED

*******************************************

SERIOUS ERROR SUMMARY FOR THE LAST TEST RUN

*******************************************

-----------------------------------------------------------------------------------------------------

See also

Detailed error log

Test preferences - Logging